|  |  |  |  |
| --- | --- | --- | --- |
| **Project Information** | | | |
| **Subrecipient or State Representative’s Name:** | | | **Floor plan:** |
| **Applicant’s Name:** | | **Co-Applicant’s Name:** | |
| **Physical Address:** | | | |
| **City:** | | **State: Texas** | **ZIP Code:** |
| **Builder Name:** | | | |
| ***\*\*Must Be Completed Immediately Prior to TREC Inspection\*\**** | | | |
| **General Inspection** | | | |
| Yes No N/A | House numbers installed. | | |
| Yes No N/A | Driveway pad is size 14’ x 20.’ Connection to street 9’ wide, where applicable. | | |
| Yes No N/A | All flatwork (driveway, walks, etc.) level, not cracked/damaged/irregular, pitting, spalling, expansion joints present. | | |
| Yes No N/A | Peepholes on all exterior doors. | | |
| Yes No N/A | Exterior door locks are properly adjusted, deadbolt fully extends into jamb. | | |
| Yes No N/A | No-step entrance serviced by ramp (if applicable) slope is 1:12 w/ two (2) grip rails. | | |
| Yes No N/A | Top of grip rails at consistent height, 34-38 inches vertically above walking surfaces, stair noses, and rampsurfaces. (ADA 2010, 504.4) | | |
| Yes No N/A | Maximum 4-inch opening on all balusters/rail supports (if applicable). | | |
| Yes No N/A | Accessible route present from street to one entrance door. | | |
| Yes No N/A | At least one entrance door with standard 36-inch door. | | |
| Yes No N/A | Exterior is free of trash and construction materials. | | |
| Yes No N/A | Foundation cables properly stressed and secured (if applicable). | | |
| Yes No N/A | Porch/decks and ramps cleaned/pressure washed. | | |
| Yes No N/A | Hallways at least 36” wide, level & ramped/beveled changes at each door threshold. | | |
| Yes No N/A | Roof complete with drip edge, all vent boot/caps, shingles straight and level. | | |
| Yes No N/A | All weatherproofing installed at exterior doors. | | |
| Yes No N/A | Building permit, Certificate of Occupancy, Elevation Certificate and Inspection green tags on site and visible. | | |
| Yes No N/A | Termite treatment completed and certificate on hand. | | |
| Yes No N/A | Green (Energy) Standards Certificate on hand. | | |
| **Inspector Observation Remarks:** | | | |
| **Exterior Inspection** | | | |
| Yes No N/A | All piping/drain lines secured to home and exposed pipes insulated. | | |
| Yes No N/A | Appropriate water main cut-off exists. | | |
| Yes No N/A | Hardie plank installed under house, painted (elevated homes where applicable). | | |
| Yes No N/A | Two (2) hose bibs with vacuum breakers (anti-syphon devices) near front and back. | | |
| Yes No N/A | Check electrostatic grounding of gas lines. | | |
| Yes No N/A | All Siding is free of blemishes. Note any cracks, dents, bows, chips or gaps. | | |
| Yes No N/A | All exposed surfaces painted without visible defects (from 6 feet away). | | |
| Yes No N/A | Silicone caulk present at exterior door sills and windows. All Exterior penetrations are weatherproofed. | | |
| Yes No N/A | All screens installed, not damaged/torn. | | |
| Yes No N/A | All Roof jacks painted to match. | | |
| Yes No N/A | Finish grade at foundation provides positive drainage away from structure, starting at a min of 6” below finish floor at slab on grade or a min of 6” below pier footings for elevated floor. | | |
| Yes No N/A | Trees trimmed at least 3 feet from the structure/roof, and sod is in required area. | | |
| **Interior Inspection** | | | |
| Yes No N/A | Inside of home is free from debris, swept and clean. | | |
| Yes No N/A | Operable switches, circuit breakers & thermostat no higher than 48” above floor. | | |
| Yes No N/A | All switches and receptacles properly installed and operable; switch plates level, flush, and without defects. Each receptacle/plug is at least 15” above the floor. | | |
| Yes No N/A | Wall and ceiling sheetrock is free of deficiencies; ridges, bubbling, cracking at tape joints, corners and lines are straight. | | |
| Yes No N/A | Verify all base trim is matching profile. Base appears to be straight; a bow in the base is a visual cue drywall is bowed. | | |
| Yes No N/A | Ensure cabinets are straight and line up with the walls properly. | | |
| Yes No N/A | Smoke/CO detectors installed in proper locations and operational. | | |
| Yes No N/A | Ensure paint coverage is acceptable, free from flaws visible from 6 feet away. | | |
| Yes No N/A | Ensure interior doors are at least standard 32” door, unless the door provides access only to closet of less than 15 square feet in area. | | |
| Yes No N/A | Check vinyl flooring for deficiencies such as peeling/lifting, visible gaps/seams, ridges/depressions, scratches, or overall poor workmanship. | | |
| Yes No N/A | Ceramic/porcelain tile – all joints perpendicular & parallel to walls. Installed around outlets, fixtures, pipes/fittings so that plates, escutcheons, and collars overlap cuts. | | |
| Yes No N/A | Check for Hot-Cold control reversal in all showers, tubs, and sinks. | | |
| Yes No N/A | Check for leaks in supply and drain lines under sinks. | | |
| Yes No N/A | Toilets flush properly and are firmly seated in place (no movement). | | |
| Yes No N/A | AC & Heat; check for cold and hot air movement; system in good working order; check thermostat functions. | | |
| Yes No N/A | AC filter in place; filter panel easily removable. | | |
| Yes No N/A | AC registers properly installed (no gaps, all screws) and level. | | |
| Yes No N/A | Septic system installed and operational (if applicable). | | |
| Yes No N/A | Well water system installed and operational (if applicable). | | |
| Yes No N/A | Water heater installed, operational. (If located on main floor in construction plans, must be in designated and properly ventilated closet.) | | |
| Yes No N/A | Appliances installed, operational. | | |
| Yes No N/A | Anti-tip device installed for the stove/oven range. | | |
| Yes No N/A | Washing machine outlet box, ice maker outlet box, dryer vent box (or trim) present. | | |
| Yes No N/A | Attic- Verify insulation installed, stop, and access door insulation are present. | | |
| Yes No N/A | Windows & doors operate smoothly (hinge screws installed, locks & hardware). | | |
| **Electrical Inspection** | | | |
| Yes No N/A | Air Conditioner breaker properly sized. | | |
| Yes No N/A | All exhaust fans and ceiling fans are operational, no excessive noise or vibration. | | |
| Yes No N/A | AC Condenser location on concrete pad or deck. Water diverter over AC unit. | | |
| Yes No N/A | Breaker box located on 1st floor, operational parts no higher than 48” from floor. | | |
| Yes No N/A | Check that all required GFCI circuits are present and operating properly. | | |
| Yes No N/A | Check that all required AFCI circuits are present and operating properly. | | |
| Yes No N/A | All circuit breakers clearly labeled. | | |
| Yes No N/A | Check ground and polarity of all receptacles. | | |
| **Inspector Observation Remarks:** | | | |
| **Accessibility Inspection (when applicable)** | | | |
| Yes No N/A | If lift present, ensure it is operable, and lift gates fasten securely. | | |
| Yes No N/A | Walk-in shower. | | |
| Yes No N/A | Grab bars installed properly. | | |
| Yes No N/A | Toilets exactly at 18 inches (on center) from finished side wall. | | |
| Yes No N/A | Toilet seat height is 17–19 inches from floor. | | |
| **Inspector Observation Remarks:** | | | |
| **Signatures** | | | |
| Under penalties of perjury, I certify that the information presented in this Affidavit is true and accurate to the best of my knowledge and belief. I further understand that providing false representations herein constitutes an act of fraud. False, misleading or incomplete information may result in my ineligibility to participate in Programs that will accept this Affidavit. 18 U.S.C. Section 1001 states that a person is guilty of a FELONY if he/she knowingly and willfully makes false statements to any department of the United States Government. | | | |
| **Inspector’s Printed Name:** | | | **Date:** |
| **Inspector’s Signature:** | | |
| **Superintendent’s Printed Name:** | | | **Date:** |
| **Superintendent’s Signature:** | | |
| **Applicant’s Printed Name:** | | | **Date:** |
| **Applicant’s Signature:** | | |
| **Co-Applicant’s Printed Name:** | | | **Date:** |
| **Co-Applicant’s Signature:** | | |

\*\*Based upon IRC 2012, ADA 2010, HUD Housing Quality Standards and CDR Design Standards.

***Disclaimer:*** *The Texas General Land Office has made every effort to ensure the information contained on this form is accurate and in compliance with the most up-to-date CDBG-DR and/or CDBG-MIT federal rules and regulations, as applicable. It should be noted that the Texas General Land Office assumes no liability or responsibility for any error or omission on this form that may result from the interim period between the publication of amended and/or revised federal rules and regulations and the Texas General Land Office's standard review and update schedule.*